## Doors

#### Front Door Glass Outer Weatherstrip Replacement

20-151

Front Door Weatherstrip Replacement

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the door.

1. Starting at the rear, pry the door glass outer weatherstrip (A) up to detach the clips (B, C) and pull the weatherstrip rearward, then remove the weatherstrip.

   Fastener Locations
   B : Clip, 4 | C : Clip, 1

2. Install the weatherstrip in the reverse order of removal and replace any damaged clips.

NOTE:

- Take care not to scratch the door.
- Use a clip remover to remove the clips.

1. At the front pillar, remove the door stop mounting bolt (A).

   Fastener Locations
   A : Bolt, 1 | B : Clip, 1 | C : Clip, 17

2. Detach the clips (B, C) and pull out the door weatherstrip (D) from the holder areas (E), then remove it.
3. Install the weatherstrip in the reverse order of removal and note these items:

- Replace any damaged clips.
- Make sure the weatherstrip is installed in the holder (F) securely.
- Apply liquid thread lock to the door stop mounting bolt before installation.
- Check for water leaks (see step 7 on page 20-163).