## Power Steering

#### Steering Gearbox Overhaul (cont'd)

17-40

Special Tools Required

- Cylinder end seal remover attachment, 07NAD-SR30200
- Driver, 27 mm, 07ZAF-S5A0100
- Valve seal ring sizing tool, 07NAG-SR30900
- Sleeve seal ring guide, 07YAG-S2X0100
- Sleeve seal ring sizing tool, 07ZAG-SA50100
- Attachment, 32 x 35 mm, 07746-0010100
- Driver, 07749-0010000
- Piston seal ring guide, 07GAG-SD40100
- Piston seal ring sizing tool, 07GAG-SD40200
- Pincers, Oetiker 1098 or equivalent, commercially available.
- Pilot collar, 07GAF-PH70100
- Locknut wrench, 07ZAA-S5A0100
- Driver handle, 07NAD-SR30101
- Seal slider, 07974-6890801
- Valve seal ring guide, 07ZAG-S5A0200

NOTE: Refer to the Exploded View as needed during this procedure.

Removal

1. Remove the steering gearbox (see page 17-35).

Disassembly

2. Unbend the lock washer (A).

3. Hold the bracket (A) with one wrench, and unscrew both rack ends (B) with another wrench. Remove the lock washers.

4. Remove cylinder lines (A) from the gearbox.

5. Drain the fluid from the cylinder fittings by slowly moving the steering rack back and forth.