## Front Bulkhead

#### Removal

3-5

Installation

1. BULKHEAD UPPER FRAME
2. BULKHEAD SIDE
3. FRONT DAMPER EXTENSION
4. WHEELHOUSE UPPER MEMBER
5. FRONT WHEELHOUSE
6. FRONT SIDE FRAME
7. BULKHEAD SIDE STAY
8. FRONT LOWER CROSS-MEMBER

1. Set the new front bulkhead into position and measure the front compartment diagonally. Check the body dimensions (see section 4).
2. Tack weld the clamped position.
3. Temporarily install the hood, front fender, headlight and front bumper and check for differences in level and clearance.
4. Perform the main welding:

1. BULKHEAD UPPER FRAME
2. FRONT DAMPER EXTENSION
3. WHEELHOUSE UPPER MEMBER
4. BULKHEAD SIDE
5. FRONT SIDE FRAME
6. FRONT LOWER CROSS-MEMBER
7. FRONT WHEELHOUSE
8. BULKHEAD SIDE STAY
9. FRONT SIDE FRAME