## Engine Assembly

#### Engine Removal (cont'd)

5-7

19. Remove the alternator (see page 4-31).

20. Remove the air conditioning (A/C) hose bracket (A) and P/S hose bracket (B).

21. Remove the alternator lower bracket (A), then remove the A/C compressor (B) without disconnecting the A/C hoses.

22. Remove the radiator cap.
23. Raise the hoist to full height.
24. Remove the front tyres/wheels.
25. Remove the splash shield.

26. Loosen the drain plug in the radiator, drain the engine coolant (see page 10-8).
27. Drain the transmission fluid. Reinstall the drain plug using a new washer:

- Manual transmission (see page 13-3).
- Automatic transmission (see page 14-122).
- Honda multi matic (see page 14-312).

28. Drain the engine oil. Reinstall the drain bolt using a new washer (see page 8-5).