## Driveline/Axle

#### Driveshaft Disassembly (cont'd)

16-7

8. Wrap the splines on the driveshaft with vinyl tape (A) to prevent damage to the boot and dynamic damper.

1. (Except right driveshaft on SOHC engines A/T models)

1. Remove the inboard boot and dynamic damper. Take care not to damage the boot and dynamic damper.
2. Remove the vinyl tape.

Outboard Joint Side:

1. Remove the boot bands. Take care not to damage the boot and dynamic damper.

- If the boot band is an ear clamp type (A), lift up the three tabs (B) with a screwdriver.

Ear Clamp Type

2. Slide the outboard boot (A) to the inboard joint side. Take care not to damage the boot.