## SRS

#### Precautions and Procedures (cont'd)

23-31

Disconnecting the Airbag Connectors, Side Airbag Connectors and Seat Belt Tensioner Connectors

Before removing a front airbag, side airbag or other SRS related devices (the SRS unit, the cable reel, the side impact sensors and the seat belt tensioner connector), disconnecting connectors from related devices, or removing the dashboard or the steering column, disconnect the airbag connectors or the side airbag connectors to prevent accidental deployment.

Turn the ignition switch OFF and disconnect the negative cable from the battery, and wait at least 3 minutes before beginning the following procedures.

- Before disconnecting the dashboard wire harness B 18P connector (A) from the SRS unit, disconnect the driver's airbag 2P connector (C), the front passenger's airbag 2P connector (D), the left side seat belt tensioner 2P connector (F) and the right side seat belt tensioner 2P connector (G).
- Before disconnecting the floor wire harness 18P connector (I) from the SRS unit, disconnect both side airbag 2P connectors (L, M).
- Before disconnecting the cable reel 4P connector (B), disconnect the driver's airbag 2P connector (C).
- Before disconnecting the floor wire harness 4P connector (E), disconnect both seat belt tensioner 2P connectors (F, G).