## Interior Trim

#### Carpet Replacement (cont'd)

20-213

3. Remove the parking brake cover (A).

- Remove the clip (B).
- Pull up the rear portion on the cover to release the clips (C).
- If equipped, disconnect the front seat heater switch connectors (D).

  Fastener Locations
  B : Clip, 1 | C : Clip, 2

4. Using a utility knife, cut the carpet (A) under the heater area (B) on the driver's side, then pull back the carpet.

5. Remove the clips (A) and release the fasteners (B), then remove the carpet (C).

   Fastener Locations
   A : Clip, 3