## Cooling System

#### Radiator Replacement (cont'd)

10-13

1. Pull up the radiator, then remove the fan shroud assemblies and other parts from the radiator.

1. INTERCOOLER INLET HOSE
2. UPPER RADIATOR HOSE
3. INTERCOOLER OUTLET HOSE
4. INTERCOOLER
5. RADIATOR FAN SWITCH A

   24 Nm (2.4 kgf/m, 17 lbf/ft)

6. O-RING

   Replace.

7. RADIATOR FAN SWITCH B

   24 Nm (2.4 kgf/m, 17 lbf/ft)

8. RADIATOR
9. O-RING

   Replace.

10. DRAIN PLUG
11. LOWER CUSHION
12. LOWER RADIATOR HOSE
13. A/C CONDENSER FAN ASSEMBLY
14. RADIATOR FAN ASSEMBLY

1. Install the radiator in the reverse order of removal. Make sure the upper and lower cushions are securely.

1. Install the bulkhead in the reverse order of removal. Apply body paint to the bulkhead mounting bolts.

a a a