## Air Conditioning

#### Symptom Troubleshooting Index

21-68

4-door, 5-door KE Model

Symptom | Diagnostic procedure | Also check for
Condenser fan does not run at all (but radiator fan runs with the A/C on) | Condenser Fan Circuit Troubleshooting (see page 21-74) |

- Blown fuse No. 1 (20A) in the under-hood fuse/relay box and No. 14 (10A) in the under-dash fuse/relay box
- Poor ground at G201
- Cleanliness and tightness of all connectors

Both fans do not run with the A/C on | Radiator and Condenser Fans Common Circuit Troubleshooting (see page 21-75) |

- Blown fuse No. 1 (20A) and No. 4 (20A) in the under-hood fuse/relay box and No. 14 (10A) in the under-dash fuse/relay box
- Poor ground at G201
- Cleanliness and tightness of all connectors

Compressor clutch does not engage | Compressor Clutch Circuit Troubleshooting (see page 21-76) |

- Blown fuse No. 1 (20A) in the under-hood fuse/relay box and No. 14 (10A) in the under-dash fuse/relay box
- Cleanliness and tightness of all connectors

A/C System does not come on (both fans and compressor) | A/C Pressure Switch Circuit Troubleshooting (see page 21-78) |

- Cleanliness and tightness of all connectors