## Power Windows

#### Passenger's Switch Replacement

22-201

4-door:

1. Remove the door grip cover (see page 20-7).
2. Remove the screws and passenger's power window switch (A).
   NOTE: The illustration shows front passenger's door.

3. Disconnect the 5P connector (B) from the switch.

5-door (Front Passenger's):

1. Remove the door grip cover (see page 20-144).
2. Remove the screws and passenger's power window switch (A).

3. Disconnect the 5P connector (B) from the switch.
4. Remove the screws and switch (A) from the switch panel (B).