## Dashboard

#### Steering Hanger Beam Replacement

20-226

NOTE: Put on gloves to protect your hands.

1. Remove the dashboard (see page 20-223).
2. Remove the these items from the dashboard:

- Instrument panel (see page 20-215)
- Driver's pocket (see page 20-216)
- Gauge assembly (see page 22-93)
- Centre panel, auto A/C (see page 20-219)
- Sunlight sensor, auto A/C (see page 21-152)
- Passenger's airbag (see page 23-167)

3. Remove the screws, then remove the glove box striker (A). If equipped, disconnect the glove box light connector (B).

   Fastener Locations
   : Screw, 4

4. Loosen the bolts (A) and remove the bolt (B) and pull down the under-dash fuse/relay box (C) to release the bracket (D).

Fastener Locations
A : Bolt, 2 | B : Bolt, 1

5. Remove the sunlight sensor wire harness (A) by removing the cushion tape (B).