## Design Specifications

#### (cont'd)

2-34

Item | Measurement | Qualification | Specification
TYRES (5-door (England made) model) | Size of front, rear and spare for KE model | 1.4S, 1.4SE | 185/70R14 88H
1.4SE Executive, 1.6S, 1.6SE, 1.6SE Executive | 195/60R15 88H
Size of front and rear for KG, KR, KS models | 1.4S, 1.4LS | 185/70R14 88H
1.6S, 1.6LS, 1.6ES | 195/60R15 88H
Size of spare for KG, KR, KS models |  | T125/70D15 95M
Size of front, rear and spare for KY model |  | 195/60R15 88H
TYRES (Coupe model) | Size of front and rear tyre | KK, KX models | P185/65R15 86H
KE, KG, KB, KR, KY models | P195/60R15 88H
Size of spare tyre | KG, KB, KR, KX models | T125/70D15 95M
AIR CONDITIONING | Cooling capacity |  | 3,870 kcal/h (15,400 BTU/h)
Compressor | Type/manufacturer | Scroll/SANDEN
Number of cylinders | -
Capacity | 85.7 ml/rev. (5.23 cu in./rev.)
Maximum speed | 12,000 rpm
Lubricant capacity | 130 ml (4 1/3 fl oz)
Lubricant type | SP-10 (P/N 38897-P13-003, 38898-P13-003 or 38899-P13-A01)
Condenser | Type | Corrugated fin
Evaporator | Type | Corrugated fin
Blower | Type | Radial fan
Motor type | 190 W/12 V
Speed control | 9-speed
Maximum capacity | 480 m3/h (16,900 cu ft/h)
Temperature control |  | Air-mix type
Compressor clutch | Type | Dry, single plate, poly-V belt drive
Electrical power consumption at 20°C (68°F) | 42 W maximum at 12 V
Refrigerant | Type | HFC-134a (R-134a)
Quantity | 500-550 g (17.5-19.5 oz)

a a a