## Conventional Brake Components

#### Brake Booster Replacement

19-11

1. Remove the master cylinder (see page 19-9).

1. Remove the air cleaner mounting base (A).

1. Disconnect the vacuum hose (B) from the brake booster.

1. Remove the clip (A) and the joint pin (B) and disconnect the yoke from the brake pedal.

1. Remove the brake booster mounting flange nuts (C).

1. Remove the brake booster (A) from the engine compartment.

1. Install the brake booster in the reverse order of removal and note these items:

- Adjust the pushrod clearance before installing the brake booster.
- Use a new clip whenever installing.
- After installing the brake booster and master cylinder, fill the reservoir with new brake fluid, bleed the brake system and adjust the brake pedal height and free play.

a a a