## Starting System

#### Starter Overhaul (cont'd)

4-14

1. Measure the inside diameter of bearing on the rear cover. If measurement is more than limit, replace the rear cover assembly.

Inside diameter:

Standard:

12.018 – 12.029 mm

(0.4731 – 0.4736 in.)

Limit:

12.129 mm (0.4775 in.)

1. Measure the inside diameter of the centre bracket (p). If measurement is more than limit, replace the centre bracket (P).

Inside diameter:

Standard:

18.035 – 18.060 mm

(0.7100 – 0.7110 in.)

Limit:

18.160 mm (0.7150 in.)

1. Measure the inside diameter of bearing on the pinion shaft. If measurement is more than limit, replace the pinion shaft.

Inside diameter:

Standard:

6.725 – 6.77mm (0.2648 – 0.2665 in.)

Limit:

6.87 mm (0.2705 in.)

a a a