## Honda Multi Matic Transmission/CVT

#### Pressure Tests

14-316

Special Tools Required

- A/T oil pressure gauge set, 07406-0020004
- A/T low pressure gauge, 07406-0070001

1. Before testing, be sure the transmission fluid is filled to the proper level.
2. Raise the front of the vehicle and make sure it is securely supported.
3. Set the parking brake and block rear wheels securely.
4. Allow the front wheels to rotate freely.
5. Warm up the engine (the radiator fan comes on), then stop it and connect the tachometer.
6. Connect the oil pressure gauges to each inspection hole and do not allow dust or other foreign particles to enter the holes.

TORQUE: 18 Nm (1.8 kgf/m, 13 lbf/ft)

NOTE:

- Drive pulley pressure may be above 3,430 kPa (3.43 MPa, 35.0 kgf/cm2, 498 psi) when there is a transmission problem that causes the PCM to go into the fail-safe mode.
- Use a commercially available oil pressure gauge that measures 4,900 kPa (4.90 MPa, 50.0 kgf/cm2, 711 psi) or more and use the A/T oil pressure gauge set and the A/T low pressure gauge.

A/T OIL PRESSURE GAUGE SET, 07406-0020004

A/T LOW PRESSURE GAUGE, 07406-0070001