## Glass

#### Windshield Replacement (cont'd)

20-178

13. Glue the rubber dams (A), fasteners (B) to the inside face of the windshield (C) as shown:

- Be sure the rubber dam and fasteners line up with the alignment marks (D).
- Be careful not to touch the windshield where adhesive will be applied.

14. Glue the moulding (A) with adhesive tape (B) to the upper edge of the windshield (C):

- Be sure the alignment mark (D) of the moulding lines up with the alignment mark (E) of the windshield.
- Be careful not to touch the windshield where adhesive will be applied.

15. Install the fasteners (A), retainers (B, C) and clips (D) to the body.

    Fastener Locations
    A : Fastener, 6 | B : Retainer, 2

    C : Retainer, 6 | D : Clip, 2