## Automatic Transmission

#### Transmission Installation

14-130

1. Install the starter (A) on the torque converter housing (B).

2. Install the torque converter assembly (C) on the mainshaft (D) with a new O-ring (E).
3. Install the 14 mm dowel pins (F) in the torque converter housing.
4. Place the transmission on a jack and raise it to the engine level.
5. Attach the transmission to the engine, then install the rear mount/bracket (A) with the mount/bracket bolts (B) and the transmission housing mounting bolt (C).

6. Install the transmission housing mounting bolts.

7. Install the transmissioNmount bracket (A).

Tighten the bolt (B) loosely and tighten the nuts (C) to the specified torque, then tighten the bolt to the specified torque.