## Roof Panel

#### Installation

3-25

1. Set the new roof panel into position and clamp it. Check the body dimensions (see section 4), and check the width of the roof moulding installation.
2. Install the roof arch gusset, and tack weld the roof panel.
3. Temporarily install the windshield, door and rear window and check for difference in level and clearance.
4. Perform the main welding.

1. OUTER PANEL
2. ROOF PANEL
3. ROOF SIDE RAIL

VIEW (Z)

1. ROOF ARCH GUSSET

5. From inside the vehicle, plug weld the front pillar inner upper, rear inner panel and front and rear roof rails.

1. FRONT INNER UPPER PILLAR
2. FRONT ROOF RAIL
3. REAR INNER PANEL
4. REAR ROOF RAIL