## Cylinder Head

#### Crankshaft Pulley Removal and Installation

6-12

Special Tools Required

- Handle, 07JAB-0010200
- Pulley holder attachment, HEX 50 mm, 07JAB-0010400
- Socket wrench, 19 mm, 07JAA-0010200

Removal

1. Remove front tyres/wheels.

1. Remove the splash shield (see step 21 on page 5-6).

1. Hold the pulley with handle (A) and holder attachment (B).

1. Remove the bolt with a 19 mm socket (C) and breaker bar.

Installation

1. Clean the crankshaft pulley (A), crankshaft (B), bolt (C) and washer (D). Lubricate as shown below.

O: Clean

: Lubricate

1. Install the crankshaft pulley and hold the pulley with handle (A) and holder attachment (B).

1. Tighten the bolt to 245 Nm (25.0 kgf/m, 181 lbf/ft) with a torque wrench and 19 mm socket (C). Do not use an impact wrench.

1. Install the splash shield (see step 18 on page 5-14).

1. Install front tyres/wheels.

a a a