## Seats

#### Rear Seat-back Cover Replacement (cont'd)

20-42

4. Pull back the seat-back cover (A) and remove the clips (B) and release the hooks (C).

Fastener Locations

B : ClipLeft, 6

Right, 3

Left seat back:

Right seat back:

5. Remove the seat-back cover and pad (D) from the seat-back frame (E).

6. Pull back the edge of the seat-back cover (A) all the way around and remove the clips (B), then remove the seat-back cover.

Left seat back:

Right seat back:

7. Install the cover in the reverse order of removal and note these items:

- To prevent wrinkles when installing a seat-back cover, make sure the material is stretched evenly over the pad before securing the hooks and clips.
- Replace any clips you removed with new ones. Install them with commercially available upholstery ring pliers.