## SRS

#### SRS Indicator Light Circuit Troubleshooting (cont'd)

23-162

31. Connect the No. 3 terminal of the U1o connector and the No. 5 terminal of U3o connector with a jumper wire.

U3o CONNECTOR

Wire side of female terminals

32. Turn the ignition switch ON (II).
33. Check the SRS indicator light.

Does the SRS indicator light go off?

YES - Faulty SRS unit; replace the SRS unit.

NO - Go to step 34.

34. Turn the ignition switch OFF.
35. Disconnect the jumper wire between the No. 3 terminal of the dashboard wire harness B 18P connector and the No. 5 terminal of the U3o connector.
36. Check the No. 13 (10A) fuse in the under-dash fuse/relay box.

Is the fuse OK?

YES - Go to step 40.

NO - Go to step 37.

37. Replace the No. 13 (10A) fuse in the under-dash fuse/relay box.

38. Disconnect the C1 connector (A) from the gauge assembly.

39. Check resistance between the No. 5 terminal of the U3o connector and body ground. There should be 1 M ohm or more.

U3o CONNECTOR

Wire side of female terminals

Is the resistance as specified?

YES - Faulty SRS indicator light circuit in the gauge assembly; replace the gauge assembly.

NO - Short to ground in the floor wire harness or in dashboard wire harness A; replace the faulty harness.