## Engine Assembly

#### Engine Installation (cont'd)

5-15

1. Install the shift cables using the plastic washers (A), washers (B), new cotter pins (C) and change wire plate (D).

1. Install the clutch slave cylinder (A) and clutch line bracket mounting bolt (B).

1. Install the battery base (A), then install the harness clamps (B) and ground cable (C).

1. Install the air cleaner housing (A) and intake air duct (B), then connect the mass air flow (MAF) sensor connector (C) and install the vacuum hose (D).

a a a