## A/T Gear Position Indicator

#### Transmission Range Switch Test (cont'd)

14-160

5-door Model

1. Remove the transmission range switch harness connector (A) from the connector bracket (B), then disconnect the connector.

Connector Terminal Description

No. | Description | No. | Description
1 | GND | 6 |
2 | Not used | 7 |
3 | ATP NP | 8 |
4 |  | 9 |
5 | Not used | 10 |

2. Check for continuity between terminals at the harness connector. There should be continuity between the terminals listed for each switch position.

In position, between terminals:

- No. 1 and No. 3
- No. 1 and No. 8
- No. 3 and No. 8

In position, between terminals:

- No. 1 and No. 9

In position, between terminals:

- No. 1 and No. 3
- No. 1 and No. 10
- No. 3 and No. 10

In position, between terminals:

- No. 1 and No. 4

In position, between terminals:

- No. 1 and No. 6

In position, between terminals:

- No. 1 and No. 7

3. If there is no continuity between any terminal, remove the transmission range switch cover and disconnect the connector (A) at the switch (B).

Connector Terminal Description

No. | Description | No. | Description
1 |  | 6 |
2 |  | 7 |
3 |  | 8 |
4 | GND | 9 | Not used
5 | ATP NP | 10 | Not used

4. Check for continuity between terminals at the switch connector (C). There should be continuity between the terminals listed for each position.

In position, between terminals:

- No. 4 and No. 5
- No. 4 and No. 6
- No. 5 and No. 6

In position, between terminals:

- No. 1 and No. 4

In position, between terminals:

- No. 4 and No. 5
- No. 4 and No. 7
- No. 5 and No. 7

In position, between terminals:

- No. 2 and No. 4

In position, between terminals:

- No. 4 and No. 8

In position, between terminals:

- No. 3 and No. 4
- If there is no continuity between any terminals, check the transmission range switch installation. If the transmission range switch installation is OK, replace the switch.
- If the transmission range switch continuity check was OK, replace the faulty transmission range switch harness.