## Stereo Sound System

#### Audio Unit Connector Replacement

22-212
Audio Unit Removal/Installation

Cavity

Wire | Connects to
1*¹ | YEL/GRN | Roof antenna
2 | YEL/RED | ACC (Main stereo power supply)
3 | ——— | Not used
4*² | RED/WHT | Security signal input
5 | PNK | Right rear[door]speaker (+)
6 | BLU/WHT | Left rear [door] speaker (+)
7 | GRN/YEL | Right front door speaker (+)
8 | GRN/BLK | Left front door speaker (+)
9 | RED/BLK | Lights - on signal
10 | WHT/RED | Constant power
11 | ——— | Not used
12 | ——— | Not used
13 | ——— | Not used
14 | ——— | Not used
15 | BLU/YEL | Right rear [door] speaker ( – )
16 | BLU/BLK | Left rear [door] speaker ( – )
17 | GRY/RED | Right front door speaker ( – )
18 | LT GRN | Left front door speaker ( – )
19*³ | RED | Dash lights brightness controller
20 | BLK | Ground (G503)

[ ]: 5-door

*1: 5-door with roof antenna

*2: With security alarm system

*3: With dash lights brightness controller

AUDIO UNIT 20P CONNECTOR

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the dashboard and related parts.

1. Make sure you have the anti-theft code for the radio, then write down the frequencies for the radio's preset buttons.
2. Remove the dashboard centre lower cover (see page 20-77).
3. Remove the heater control panel (or climate control unit) (see page 21-51) from the centre panel.
4. Remove the four mounting bolts and the audio unit from the radio brackets.

5. Install the audio unit in the reverse order of removal and note these items:

- Make sure the audio unit and A/C connectors are plugged in properly and the antenna lead is connected properly.
- Enter the anti-theft code for the radio, then enter the customer's radio station presets.