## Cylinder Head

#### Timing Belt Installation (cont'd)

6-23

5. Install the CKP sensor.

6. Install the all bolts loosely, then tighten the mounting bolts as the numbered sequence shown.

7. Install the lower cover.

8. Clean the pulley bolt and washer.
9. Clean all oil off the inside face (A) of the crankshaft pulley and apply lubricant to the pulley bolt (B) and washer (C).

O: Clean

X: Remove any oil

: Lubricate