## Front Suspension 20

#### Damper/Spring Replacement

18-20

Exploded View

1. SELF-LOCKING NUT

   12 x 1.25 mm, 44 Nm (4.5kgf/m, 33 lbf/ft), Replace.

2. UPPER SPRING SEAT
3. UPPER SPRING MOUNTAIN CUSHION

   NOTE: Do not remove the cushion from the spring. Replace it with a new one if it was removed from the spring.

   Set the new cushion on the spring with the projection of the cushion and the upper end of the spring in the position shown. The cushion has the six claws. Secure the cushion against the spring by bending the three claws (marked with) out of six securely.

4. BUMP STOP

   Check for weakness and damage.

5. DAMPER UNIT

   Check for oil leak, gas leak and smooth operation.

6. DAMPER SPRING

   Check for free length.

7. UPPER SPRING MOUNTING CUSHION

   Check for deterioration and damage.

8. DAMPER MOUNTING BEARING

   Check for smooth operation.

9. DAMPER MOUNTING BASE

   Check for deformation.