## Intake Manifold and Exhaust System

#### Intake Manifold Removal and Installation

9-2

NOTE: Use a new O-rings and gasket when reassembling.

1. O-RING

   Replace.

2. MANIFOLD ABSOLUTE PRESSURE (MAP) SENSOR
3. THROTTLE BODY
4. O-RING

   Replace.

5. INJECTOR BASE STIFFENER
6. GASKET

   Replace.

7. INJECTOR BASE
8. INTAKE MANIFOLD BRACKET
9. O-RINGS

   Replace.

10. INTAKE MANIFOLD

    Replace if cracked or if mating surfaces are damaged.