## Frame

#### Frame Repair Chart

20-134

Top View

Unit: mm (in) | a | For sub-frame Ø15 (0.59) | e | For damper mount Ø11.5 (0.45)
Ø: Inner diameter | b1 | For engine mount Ø13 (0.51) | f | Damper centre Ø78 (3.07)
| b2 | For engine mount Ø13 (0.51) | g | For damper mount Ø11.5 (0.45)
| b3 | For engine mount Ø13 (0.51) | h | For damper mount Ø11.5 (0.45)
| c1 | For transmission mount Ø13 (0.51) | i | For sub-frame Ø11 (0.43)
| c2 | For transmission mount Ø13 (0.51) | j | For sub-frame Ø15 (0.59)
| c3 | For transmission mount Ø13 (0.51) | k | For sub-frame Ø25 (0.98)
| d1 | For transmission mount Ø13 (0.51) | l | For sub-frame Ø50 (1.97)
| d2 | For transmission mount Ø13 (0.51) |  |
| d3 | For transmission mount Ø13 (0.51) |  |