## Heating

#### Heater Control Panel Overhaul

21-52
Push Switch Test

Except 4-door, 5-door KE Model

1. DIALS
2. HEATER FAN SWITCH
3. BULBS
4. AIR MIX CONTROL CABLE
5. MODE CONTROL CABLE

Air Mix and Mode Control Cables Replacement

1. When installing the air mix control cable, set the temperature control dial to MAX COOL. When installing the mode control cable, set the mode control dial to VENT.
2. Attach the control cable (A) to the control lever (B) as shown.

3. Adjust the length between the inner cable (A) and the cable housing (B) of the heater unit side to 28 ±; 0.3 mm as shown.

4. Keep the length of the control cable adjusted in step 3, hold the control cable with the cable clamp.

Except 4-door, 5-door KE Model

Check for continuity between the terminals in each switch position according to the table.