## Heating

#### Blower Unit Removal and Installation (cont'd)

21-55

5-door

1. Remove the passenger's dashboard lower cover (see page 20-206), the left kick panel (see page 20-220) and the glove box (see page 20-220).
2. Cut the plastic cross brace in the glove box opening with diagonal cutters in the area shown. Remove and discard the plastic cross brace.

3. Remove the bolts and the glove box frame.

4. Remove the ECM/PCM (see page 11-3).

5. Disconnect the connectors (A) from the blower motor and the power transistor or blower resister, then remove the wire harness clips (B) and the connectors (C). Remove the self-tapping screws and the bracket (D).

6. Disconnect the connector (A) from the recirculation control motor, then remove the wire harness clip (B). Remove the mounting bolts, the mounting nuts and the blower unit (C).

7. Install the unit in the reverse order of removal. Make sure that there is no air leakage.