## Maintenance Schedule for Normal Conditions (European Model)

3-4

Listed by Distance/Time

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule on 3-6 and 3-7 do not apply.

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
miles x 1,000 | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil |  |  |  |  |  |  |  |  |  |
Replace engine oil filter |  |  |  |  |  |  |  |  |  |
Replace air cleaner element |  |  |  |  |  |  |  |  |  |
Inspect valve clearance |  |  |  |  |  |  |  |  |  |
Replace fuel filter |  |  |  |  |  |  |  |  |  |
Replace spark plugs |  |  |  |  |  |  |  |  |  |
Replace timing belt, and inspect auto-tensioner, water pump | Every 120,000 km (72,000 miles) or 96 months
Inspect and adjust drive belts |  |  |  |  |  |  |  |  |  |
Inspect idle speed |  |  |  |  |  |  |  |  |  |
Replace engine coolant | At 200,000 km (120,000 miles) or 120 months, then replace every 100,000 km (60,000 miles) or 60 months
Replace transmission fluid | Manual Transmission | Every 120,000 km (72,000 miles) or 96 months
Automatic Transmission | At 120,000 km (72,000 miles) or 96 months, then replace every 80,000 km (48,000 miles) or 48 months
CVT | At 80,000 km (48,000 miles) or 60 months, then replace every 60,000 km (36,000 miles) or 48 months
Inspect front and rear brakes |  |  |  |  |  |  |  |  |  |
Replace brake fluid | Every 36 months
Check parking brake adjustment |  |  |  |  |  |  |  |  |  |
Replace air conditioning filter | Every 30,000 km (18,000 miles) or 12 months
Check light alignment |  |  |  |  |  |  |  |  |  |
Test drive (noise, stability, dashboard operation) |  |  |  |  |  |  |  |  |  |
Visually inspect the following items:
Tie rod ends, steering gearbox and boots |  |  |  |  |  |  |  |  |  |
Suspension components
Driveshaft boots
Brake hoses and lines (including ABS)
All fluid levels and condition of fluid
Exhaust system
Fuel line and connections
Tyre condition

a a a