## Security System

#### Hood Switch Test

22-266

Security Horn Test

1. Open the hood.
2. Disconnect the 2P connector from the hood switch.

Terminal side of male terminals

3. Check for continuity between the terminals.

- There should be continuity between the No. 1 and No. 2 terminals when the hood is opened.
  (lever released)
- There should be no continuity between the No. 1 and No. 2 terminals when the hood closed.
  (lever pushed down)

1. Remove the front bumper (see page 20-105).
2. Disconnect the 1P connector from the horn.

4-door:

5-door:

3. Test the horn by connecting battery power to the terminal (A) and grounding the body ground (B).
   The horn should sound.
4. If the horn fails to sound, check for.

- faulty security horn relay.
- faulty mounting bolt.