## Interior Trim

#### Headliner Removal/Installation (cont'd)

20-212

Carpet Replacement

6. If necessary, remove the bolts, then remove the grab handle bracket (A). Remove the remaining grab handle brackets, as needed.

Fastener Locations
: Bolt, 6

7. Install the headliner in the reverse order of removal and note these items:

- When reinstalling the headliner through the door opening, be careful not to fold or bend it. Also, be careful not to scratch the body.
- Check that both sides of the headliner are securely attached to the trim.

SRS components are located in this area. Review the SRS component locations (see page 23-24) and the precautions and procedures (see page 23-25) in the SRS section before performing repairs or service.

NOTE:

- Put on gloves to protect your hands.
- Take care not to damage, wrinkle or twist the carpet.
- Be careful not to damage the dashboard or other interior trim pieces.

1. Remove these items:

- Front seats, both sides (see page 20-229)
- Rear seat cushion, both sides (see page 20-237)
- Kick panels, both sides (see page 20-206)
- Front door sill trim, both sides (see page 20-206)
- Rear door sill trim, both sides (see page 20-206)
- Dashboard centre lower cover (see page 20-217)
- Driver's dashboard under cover (see page 20-216)
- Passenger's dashboard lower cover (see page 20-220)

2. Detach the clips, then remove the footrest (A).

   Fastener Locations
   : Clip, 2