## Manual Transmission

#### Transmission Disassembly

13-15

Exploded View – Clutch Housing

1 | DIFFERENTIAL ASSEMBLY | 10 | 6 mm FLANGE BOLT | 18 | 6 mm FLANGE BOLT
2 | NEEDLE BEARING |  | 9.8 Nm (1.0 kgf/m, 7.2 lbf/ft) |  | 15 Nm (1.5 kgf/m, 11 lbf/ft)
3 | OIL GUIDE PLATE C | 11 | 6 mm FLANGE BOLT | 19 | REVERSE IDLER GEAR
4 | MAGNET |  | 15 Nm (1.5 kgf/m, 11 lbf/ft) | 20 | REVERSE GEAR SHAFT
5 | CLUTCH HOUSING | 12 | REVERSE LOCK CAM | 21 | 26 x 42 x 7 mm OIL SEAL
6 | 14 x 20 mm DOWEL PIN | 13 | 5-R SHIFT PIECE |  | Replace.
7 | 35 x 56 x 8 mm OIL SEAL | 14 | 8 mm SPRING WASHER | 22 | BALL BEARING
| Replace. | 15 | 8 mm SPECIAL BOLT | 23 | 36 mm SPRING WASHER
8 | O-RING |  | 31 Nm (3.2 kgf/m, 23 lbf/ft) | 24 | 26 mm WASHER
| Replace. | 16 | SHIFT FORK ASSEMBLY | 25 | MAINSHAFT ASSEMBLY
9 | VEHICLE SPEED SENSOR (VSS) | 17 | REVERSE SHIFT FORK | 26 | COUNTERSHAFT ASSEMBLY