## Engine Assembly

#### Engine Removal (cont'd)

5-8

39. Remove the transmission mount bracket mounting bolt/nuts.

M/T:

A/T:

40. Make sure the hoist brackets are positioned properly. Raise the hoist to full height.

41. Remove the rear mount mounting bolts.

42. Use a marker to make alignment marks on the reference lines (A) that align with the centres of the rear sub-frame mounting bolts (B).

43. Remove the front sub-frame.