## Automatic Transmission

#### Shift Lever Installation

14-80

1. Cover around the opening of the console with tape or equivalent to prevent damage to the console.
2. Install the shift lever assembly (A) in the console and secure it with the bolts (B).

3. Install the bracket (C).
4. Connect the D3 switch/shift lock solenoid connector (6P) (D) and install it on the shift lever bracket.
5. Turn the ignition switch ON (II) and verify that the position indicator light comes on.

6. If necessary, push down the shift cable until it stops, then release it. Pull the shift cable back one step so that the shift cable is in

7. Turn the ignition switch OFF.
8. Insert a 6.0 mm (0.24 in.) pin (A) into the positioning hole on the shift lever bracket base through the positioning hole on the sift lever assembly. The shift lever is secured in position.