# BACK DOOR > THREE-DIMENSIONAL DISTANCE

HINT:

1. Point F, f on the vehicle are asymmetrical.
2. In cases in which only one dimension is given, left and right are symmetrical.

1. For symbols, capital letters indicate right side of vehicle, small letters indicate left side of vehicle (seen from rear).

Measuring Point Name
Symbol | Name | Hole Diameter mm (in.)
A, a | Back Door Hinge Installation Hole | φ16 (0.63)
B, b | Back Door Stay Installation Nut | M6 (0.24)
C, c | Back Door Opening Reinforcement/Back Door Opening Reinforcement Lower Adjoining Portion | -
D, d | Quarter Panel Standard Hole | φ13 (0.51)
E, e | Back Door Opening Reinforcement Lower/Body Lower Back Panel Reinforcement Adjoining Portion | -
F, f | Back Door Lock Installation Nut | M6 (0.24)
G, g | Rear Suspension Installation Hole | φ25.5 (1.00)
H, h | Rear Absorber Mounting Bracket Standard Hole | φ10 (0.39)
J | Center Floor Pan Standard Hole | φ10 (0.39)
K, k | Center Body Pillar Assembly Mark | -