# FRONT SIDE MEMBER > ASSEMBLY REPLACEMENT (PATTERN 2)

1. With the radiator support and front fender apron removed.

REMOVAL

Symbol meaning
| Remove Weld Points

INSTALLATION

Symbol meaning
| Plug Weld
| Fillet Weld

INSTALLATION POINT

1. Temporarily install the new parts and measure each part of the new parts in accordance with the body dimension diagram. (See the body dimension diagram)
2. Make sure to attach correctly in accordance with the body dimension diagram as this part affects the front wheel alignment.
3. After welding, apply body sealer and undercoating to the corresponding parts. (See the paint / coating)
4. After applying the top coat, apply anti-rust agent to the internal panel portion of the closed section structural weld points.