# FRONT FENDER APRON > ASSEMBLY REPLACEMENT

1. With the radiator upper side support and cowl top side panel removed.

REMOVAL

Symbol meaning
| Remove Weld Points
| Remove Weld Points
| Remove Weld Points

REMOVAL POINT

1. After removing the front side member to spring support gusset, remove the front fender apron.

INSTALLATION

Symbol meaning
| Plug Weld
| Plug Weld
| Plug Weld

INSTALLATION POINT

1. Inspect the fitting of the related parts around the new parts before welding. This affects the appearance of the finish.
2. Temporarily install the new parts and measure each part of the new parts in accordance with the body dimension diagram. (See the body dimension diagram)
3. After welding the the front fender apron to the vehicle side, install the front side member to spring support gusset.
4. Make sure to attach correctly in accordance with the body dimension diagram as this part affects the front wheel alignment.
5. After welding, apply body sealer and undercoating to the corresponding parts. (See the paint / coating)
6. After applying the top coat, apply anti-rust agent to the internal panel portion of the closed section structural weld points.