# BODY PANEL ANTI-CHIPPING PAINT > APPLICATION AREAS

CAUTION:

  Work must be performed while wearing the appropriate protective gear and in a well-ventilated area.

1. To protect the body from damage due to gravel, apply the anti-chipping paint to the rocker panels, wheel arches and lower parts of the doors.

   HINT:
   1. Apply anti-chipping paint to the indicated areas first, before applying the top coat.
   2. If anti-chipping paint is unnecessarily applied to an area, apply degreasing agent to a clean cloth and clean the paint off immediately.