# COWL TOP SIDE PANEL > ASSEMBLY REPLACEMENT

1. With the cowl top side upper panel removed.

REMOVAL

Symbol meaning
| Remove Weld Points
| Remove Weld Points

REMOVAL POINT

1. After removing the *1, remove the *2.

INSTALLATION

Symbol meaning
| Remove Weld Points
| Remove Weld Points
| Plug Weld
| Plug Weld

INSTALLATION POINT

1. Divide a new part of cowl top side panel in to *1 at the weld points.
2. Attach *2 after attaching *1 to the vehicle for attaching the new part.
3. After applying the top coat, apply anti-rust agent to the internal panel portion of the closed section structural weld points.