# REAR FLOOR SIDE PANEL > ASSEMBLY REPLACEMENT

1. With the body lower back panel removed.

REMOVAL

Symbol meaning
| Remove Weld Points
| Remove Weld Points

INSTALLATION

Symbol meaning
| Plug Weld
| Plug Weld

INSTALLATION POINT

1. When welding *1, make a hole on a new part for plug welding and weld the panel with the panel behind completely.
2. After welding, apply body sealer and undercoating to the corresponding parts. (See the paint / coating)
3. After applying the top coat, apply anti-rust agent to the internal panel portion of the closed section structural weld points.