# FRONT SIDE MEMBER > CUT AND JOIN REPLACEMENT SECTIONS (SMALL AREAS)

1. With the radiator support removed.

REMOVAL

Symbol meaning
| Remove Weld Points
| Remove Weld Points
| Cut and Join Location

REMOVAL POINT

1. Carefully cut the member so not to damage *1.

   Reference Value
   Area | Measurement | Area | Measurement
   *a | 80 mm (3.15 in.) | *b | 7 mm (0.28 in.)

INSTALLATION

Symbol meaning
| Plug Weld
| Plug Weld
| Butt Weld

INSTALLATION POINT

1. Temporarily install the new parts and measure each part of the new parts in accordance with the body dimension diagram. (See the body dimension diagram)
2. After welding, apply body sealer and undercoating to the corresponding parts. (See the paint / coating)
3. After applying the top coat, apply anti-rust agent to the internal panel portion of the closed section structural weld points.