# BODY PANEL SEALING > APPLICATION AREAS

1. Be sure to apply body sealer to the body panel joints and door edges (tip of outer panel folded part), etc., to waterproof and rustproof them.

   HINT:
   1. Apply degreasing agent to a clean cloth and clean the sealer application areas.
   2. After removing the applied spot sealer from the sealer application areas using thinner or equivalent, rust-proof the areas by applying primer or equivalent. Then apply body sealer.
   3. If sealer is unnecessarily applied to an area, apply degreasing agent to a clean cloth and clean off the sealer immediately.

| Flat Finishing |  | No Flat Finishing