# REAR FLOOR PAN > ASSEMBLY REPLACEMENT

1. With the body lower back panel removed.

REMOVAL

Symbol meaning
| Remove Weld Points

REMOVAL POINT

1. After removing the rear floor side panel, remove the rear floor pan.

INSTALLATION

Symbol meaning
| Plug Weld
| Fillet Weld

INSTALLATION POINT

1. Temporarily install the new parts and measure each part of the new parts in accordance with the body dimension diagram. (See the body dimension diagram)
2. Before temporarily installing the new parts, weld the spare wheel clamp bracket, rear floor pan reinforcement and weld bolts with the standard number of welding points.
3. After welding the rear floor pan to the vehicle side, install the rear floor side panel.
4. After welding, apply body sealer and undercoating to the corresponding parts. (See the paint / coating)
5. After applying the top coat, apply anti-rust agent to the internal panel portion of the closed section structural weld points.

Reference Value
Area | Measurement | Area | Measurement
*a | 275 mm (10.83 in.) | *b | 806 mm (31.73 in.)
*c | 765 mm (30.12 in.) | *d | 264 mm (10.39 in.)
*e | 298 mm (11.73 in.) | *f | 858 mm (33.78 in.)
*g | 841 mm (33.11 in.) | *h | 282 mm (11.10 in.)
*i | 556 mm (21.89 in.) | *j | 601 mm (23.66 in.)
*k | 615 mm (24.21 in.) | *l | 651 mm (25.63 in.)