# ENGINE COMPARTMENT > THREE-DIMENSIONAL DISTANCE

HINT:

1. Point F, f on the vehicle are asymmetrical.
2. In cases in which only one dimension is given, left and right are symmetrical.

1. For symbols, capital letters indicate right side of vehicle, small letters indicate left side of vehicle (seen from rear).

Measuring Point Name
Symbol | Name | Hole Diameter mm (in.)
A, a | Front Fender Installation Nut | M6 (0.24)
B, b | Front Spring Support Standard Hole | φ12.5 (0.49)
C, c | Hood Hinge Installation Nut | M8 (0.31)
D | Cowl Top Inner Panel Center Mark | -
E, e | Front Side Member Standard Hole | φ18 (0.71)
F | Front Side Member Standard Hole | φ16 (0.63)
f | Engine Mounting Bracket Installation Nut | M12 (0.47)
G, g | Radiator Upper Support Installation Nut | M6 (0.24)
H, h | Front Bumper Reinforcement Installation Nut | M10 (0.39)
J, j | Radiator Support Standard Hole | φ10 (0.39)
K, k | Front Fender Extension Standard Hole | φ10 (0.39)
L, l | Radiator Upper Support Installation Nut | M6 (0.24)
M, m | Front Fender Installation Nut | M6 (0.24)
N, n | Radiator Upper Support Standard Hole | φ10 (0.39)