#
DTC 11

BME090267000206

DTC 11 | Coil or wiring harness between immobilizer unit and coil is open circuit.
--- | ---
POSSIBLE CAUSE | • Open circuit in coil • Poor connection of coil connector • Poor connection of immobilizer unit • Defective wiring harness between immobilizer unit and coil

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT CONNECTOR CONNECTION • Is connector of coil or immobilizer unit connected securely? | Yes | Go to next step.
No | Connect connector securely.
2 | INSPECT COIL CIRCUIT FOR CONTINUITY • Is there continuity between coil terminals A and C? | Yes | Go to next step.
No | Replace coil. (See COIL REMOVAL/INSTALLATION.)
3 | INSPECT COIL CIRCUIT FOR OPEN • Disconnect coil connector and immobilizer unit connector. • Inspect for open circuit in wiring harness:

  - Immobilizer unit D to coil A, and
  immobilizer unit F to coil C
  - Immobilizer unit D to coil C, and
  immobilizer unit F to coil A

• Is there an open?

  Note

  • Vehicle harness which is connected to immobilizer unit terminals D and F, uses a twist pair wire. Because twist pair wire does not have polarity, immobilizer unit connector terminal D may be connected to coil connector terminal A or C.
  Likewise, immobilizer unit connector
  terminal F may be connected to coil
  connector terminal A or C.

Yes
Replace immobilizer unit and reprogram immobilizer system.
(See Immobilizer Unit Replacement.)
No | Repair wiring harness between coil and immobilizer unit.