#
P POSITION SWITCH (BUILT-IN SELECTOR LEVER) INSPECTION

BME051846420201

## Continuity Inspection

1. Disconnect the negative battery cable.

2. Remove the column cover.

3. Disconnect the connector.

4. Verify that the continuity is as indicated in the table.

  • If there is any malfunction, replace selector lever. (See SELECTOR LEVER REMOVAL/INSTALLATION.)

5. Connect the connector.

6. Install the column cover.

7. Connect the negative battery cable.