#
TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR INSPECTION [JA5A-EL]

BME051719010202

1. Disconnect the coupler component.

2. Remove the oil dipstick.

3. Insert the thermometer probe into the filler tube.

4. Start the engine.

5. Measure resistance between the terminals G and H.

  • If not within the specification, replace the TFT sensor. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [JA5A-EL].) (See Automatic Transaxle Workshop Manual JA5A-EL.)

ATF temperature (°C {°F}) | Resistance (kilohm)
--- | ---
-20 {-4} | 15.87-17.54
0 {32} | 5.73-6.33
20 {68} | 2.38-2.63
40 {104} | 1.10-1.22
60 {140} | 0.56-0.62
80 {176} | 0.31-0.34
100 {212} | 0.18-0.20
120 {248} | 0.11-0.12
130 {266} | 0.09-0.10

6. Connect the coupler component.