#
RADIATOR REMOVAL/INSTALLATION [AJ]

BME011215200202

1. Disconnect the negative battery cable.

2. Drain the engine coolant. (See COOLING SYSTEM SERVICE WARNINGS.)(See ENGINE COOLANT REPLACEMENT [AJ].)

3. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

4. Remove the hood lock release lever.

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

7. Refill the engine coolant. (See ENGINE COOLANT REPLACEMENT [AJ].)

1 | Fan control module connector
2 | Resevoir hose
3 | Radiator hose
4 | Oil hose (ATX)
5 | A/C pipe stay nut
6 | Radiator bracket
7 | Air seal
8 | Radiator and cooling fan (See Radiator and Cooling Fan Removal/Installation Note.)

## Radiator and Cooling Fan Removal/Installation Note

1. Before removing/installing the radiator, move the condenser toward front of the vehicle to make a space.